
1.Version of the Driver
    Ver3.18

2.Platform of the Driver
    Win95/98
    
3.Paper Setting
    The printer driver supports 80 x 297mmˇ˘80 x 210mm and user defined size.
    
    
4.Files in installation disks
    There are three files in installation disk for Win95/98 system.
    2002cp.drv
    setup.inf
    readme.txt

5.Install specification
     Please copy the installation files to a certain folder before installing it.
  Install driver under english version Win95/98 operating system.
    (1)Ensure Win95/98 is running.
    (2)Click [Start] button.
    (3)Click [Printers] icon in [Settings] item.
    (4)Double_click [Add Printer] icon.
    (5)Click [Next] button.
    (6)Select [My Computer] or [Network Printer Server],Click [Next] button.
    (7)Click [Have Disk] button.
    (8)Confirm the path of print driver,three ways:
      ˇ¤ Print driver is in A: driver, click [OK] button.
      ˇ¤ Click [Browse] button to select the path of the driver,click               [OK] button.
      ˇ¤ Input the path of the driver, then click [OK] button.
    
    (9) Click  [Next] button.
    (10)Configure Port,click [Next] button.
    (11)Click [Next] button.
    (12)If you would like to print a test page,please select [Yes]; otherwise select [No], click [Finish] button.
    (13)Insert Win95/98 system disk ,input the path of the needed files, click [OK] button.
    


    
    
    
   




    